**MFR c-3-iii Method Changes**

The method of calculating the design day forecast was substantially the same as the method used in the currently approved plan. As discussed in MFR a-3, an attrition component was added to the large load forecast calculation in the previous 2022-2025 Capacity Supply Plan, which was retained for this plan. This attrition reduced the future anticipated load need for this category of the design day forecast. Outliers were only excluded from the dataset if there was an operational issue affecting the flows to a certain pool group. Removal of outliers was used very sparingly for load forecasting for both design day and daily load models.